PC Installation Instructions

***Note*:**  If you want to keep the mixer’s current settings, create a Scene which you can recall after the upgrade. Also, If you are using a Mac to download the update file, please see additional instructions at the bottom of the page before proceeding.

1. Download the latest firmware from the QSC website
2. Unzip the downloaded file. The extracted contents will be a pdf of these download instructions and a tar.gz file. Copy the tar.gz file onto a compatible FAT 32 USB storage device. The file on the storage device will be in the format “V2.1.5035.tar.gz”. The version number will vary depending on the release but the file will always end with extension “tar.gz”.
3. Insert the USB storage device into one of the two USB ports on the mixer’s rear panel.
4. Press the Menu button, then touch the Mixer Setup button.
5. On the Mixer Setup screen, touch the Upgrade button. A dialog box displays with some IMPORTANT information about saving the mixer’s current settings.
6. Touch the Proceed button to continue the upgrade. The mixer will boot into the Software Upgrader program. This takes a few minutes.
7. Select the upgrade file you want to use.
8. Touch the Upgrade button to begin the upgrade process. This can take up to 10 minutes.
9. When the upgrade is complete, a dialog displays indicating the upgrade was successful. Press the OK button to exit the Software Upgrader and reboot the mixer.